

**WG145-1 DATA SHEET**



**HANDRAIL WALL PROTECTION SYSTEM**

-145 mm Height

-45 mm Wall Offset

-2 mm thick ARFEN Vinyl Cover

-ARFEN Vinyl Decorative Bracket

-Continuous Aluminium Retainer

-Reinforced with TPE insert

**Specifications:**


-Impact Resistance



-Fire Resistance

-Antibacterial PVC Cover


-Perfect patterned ARFEN right and left return accessories; WG006 & WG005



-Perfect patterned ARFEN internal and external corner accessories; WG007-1 & WG007-2











****